
Gosub ExecuteSciuscia
Stop

Variable Numeric Ex1
Label ExecuteSciuscia
	For Ex1 = 1 To 9e99
		'
		Gosub WaitMotorAndRecovery
		Wait Seconds 0.5
		'
	Next
Return


' ==========================================================
'   Wait until the motor(SlotMotor) is stopped
' ==========================================================
Variable Numeric WaitMot1
Label WaitMotor
	Wait Seconds 0.1
	For WaitMot1 = 1 To 9e99
		'Exit
		Return
	Next
Return

Label WaitMotorAndRecovery
	Wait Seconds 0.1
	For WaitMot1 = 1 To 9e99
		Exit
	Next
	Wait Seconds 0.2
	Gosub WaitMotor
Return


'WATCH SequenceCmd
'WATCH s1
'WATCH UCase(SequenceCmd)
'WATCH Ex1
