
Label Loop
	
	Slot 3 = 44				' near place
	Gosub StopPump
	
    '----------------------------------	'Breakpoint
	
	Slot 5 = 60				'raise
	Gosub StopPump
	Wait Seconds 0.01	'Breakpoint
	
Goto Loop


Label StopPump
	Slot 11 = 0
Return


'EXEC Slot 1 = 1000 : Slot 2 = 1000
