
s1 = COM_ReceiveNChars(10)
's1 = COM_ReceiveUntil(CRLF)
's1 = COM_Received

For v1 = 1 To Len(s1)
	s2 = s2 + Asc(Mid(s1, v1)) + " "
Next

Print s2

Variable Numeric CurrentPos
Label ConvertToPosition
	CurrentPos = Val(Mid(s1, 4))
	CurrentPos = CurrentPos + Val(Mid(s1, 4))
	CurrentPos = CurrentPos + Val(Mid(s1, 4))
	CurrentPos = CurrentPos + Val(Mid(s1, 4))
Return

Stop


'WATCH len(BytesString)
'EXEC DestX = 12
