
For v1 = 1 To 1e99
	
	For v2 = 100 To 900 Step 10
		Slot 1 = v2
		Wait Seconds 0.01
	Next
	
	Slot 1 = 0
	Wait Seconds 0.1
	
	For v2 = 900 To 100 Step 10
		Slot 1 = v2
		Wait Seconds 0.01
	Next
	
	Slot 1 = 0
	Wait Seconds 3
	
Next


'WATCH SequenceCmd
'WATCH s1
'WATCH UCase(SequenceCmd)
