

' Cliccando sulle seguenti linee si apre il pulsante "Select next error"

Button 14 Text JoyPad RUNNING

Button 14 Text ""

Button 14 Text START

Button 12 Text "ROTATE HORZ"

Button  2 Text Home (R)


Print " Test num: " + v7 + " Errors: " + v8

s1 = s1 + "ERROR: Left level too low" + CRLF
s1 = s1 + "ERROR: Left speaker. Too much distortion on the 3rd harmonics" + CRLF
s1 = s1 + "ERROR: Too much noise" + CRLF

Load Sequence SequenceFileName


' ERROR
Print "JoyPad Error not center : X = " + Int(v1)
Print "JoyPad Error not center : Y = " + Int(v2)

' NO ERROR
Print Format(v1, "0.000") + " " + Format(v2, "0.000")
Print CRLF + " Sequence file not found: " + SequenceFileName

Stop

Variable String SequenceFileName

Label START
Return

Label ROTATE HORZ
	Beep
Return

Label Home (R)
Return



'WATCH SequenceCmd
'WATCH s1
'WATCH UCase(SequenceCmd)
